From dea0a7f9ae03eba9b2b0f53da415b057c778ba82 Mon Sep 17 00:00:00 2001
From: Zheng Bao <fishbaozi@gmail.com>
Date: Tue, 17 Nov 2015 23:50:14 +0800
Subject: documentation: Update the document about building coreboot

The previous LinuxBIOS-AMD64.tex was still working with subversion.

We need a document to give the preliminary steps to build coreboot
for a new guys.

Change-Id: I64240c8344456e724f0823680e0534cf1db4c4a8
Signed-off-by: Zheng Bao <zheng.bao@amd.com>
Signed-off-by: Zheng Bao <fishbaozi@gmail.com>
Reviewed-on: http://review.coreboot.org/4510
Tested-by: build bot (Jenkins)
Reviewed-by: Patrick Georgi <pgeorgi@google.com>
---
 Documentation/CorebootBuildingGuide.tex | 1980 +++++++------------------------
 1 file changed, 427 insertions(+), 1553 deletions(-)

(limited to 'Documentation/CorebootBuildingGuide.tex')

diff --git a/Documentation/CorebootBuildingGuide.tex b/Documentation/CorebootBuildingGuide.tex
index 5b3eacf778..dac031ae3b 100644
--- a/Documentation/CorebootBuildingGuide.tex
+++ b/Documentation/CorebootBuildingGuide.tex
@@ -6,33 +6,35 @@
 \documentclass[titlepage,12pt]{article}
 \usepackage{a4}
 \usepackage{graphicx}
+\usepackage{epsfig}
+\usepackage{epstopdf}
 \usepackage{url}
+\usepackage{color}
+% \usepackage{geometry}
 \usepackage[pdftex]{hyperref}
 % \usepackage{makeidx}
 % \makeindex
+% \geometry{left=2cm,right=2cm,top=2cm,bottom=2cm}
 
 \hypersetup{
-	urlbordercolor={1 1 1},
-	menubordercolor={1 1 1},
-	linkbordercolor={1 1 1},
-	colorlinks=false,
-	% pdfpagemode=None,  % PDF-Viewer starts without TOC
-	% pdfstartview=FitH,
-	pdftitle={coreboot on AMD64},
-	pdfauthor={Stefan Reinauer},
-	pdfsubject={coreboot configuration and build process},
-	pdfkeywords={coreboot, Opteron, AMD64, configuration, Build}
+    urlbordercolor={1 1 1},
+    menubordercolor={1 1 1},
+    linkbordercolor={1 1 1},
+    colorlinks=false,
+    % pdfpagemode=None,  % PDF-Viewer starts without TOC
+    % pdfstartview=FitH,
+    pdftitle={Coreboot Porting Guide},
+    pdfauthor={Zheng Bao},
+    pdfsubject={coreboot configuration and build process},
+    pdfkeywords={coreboot, AMD, configuration, Build}
 }
 
-
-% \newcommand{\sh}[1]{\begin{verbatim}\texttt{#1}\end{verbatim}}
-% \newcommand{\prog}[1]{\textit{#1}}
-
 \setlength{\parindent}{0pt}
+\setlength{\hoffset}{0pt}
 
-\title{coreboot on AMD64}
-\author{Stefan Reinauer $<$stepan@coresystems.de$>$}
-\date{April 19th, 2009}
+\title{Coreboot from Scratch}
+\author{Stefan Reinauer $<$stepan@coresystems.de$>$\and Zheng Bao $<$zheng.bao@amd.com$>$}
+\date{Dec 4th, 2013}
 
 \begin{document}
 
@@ -44,40 +46,7 @@
 
 \newpage
 
-%
-% 1 Abstract
-%
-
-\section{Abstract}
-
-This document targets porting coreboot to new mainboards and creating
-custom firmware images using coreboot. It describes how to build
-coreboot images for the AMD64 platform, including hypertransport
-configuration and pertinent utilities. If you are missing information or
-find errors in the following descriptions, contact
-\href{mailto:stepan@coresystems.de}{\textit{Stefan Reinauer $<$stepan@coresystems.de$>$}}
-
-
-%
-% 2 Changes
-%
-
-\section{Changes}
- \begin{itemize}
- \item 2009/04/19 replace LinuxBIOS with coreboot
- \item 2004/06/02 url and language fixes from Ken Fuchs $<$kfuchs@winternet.com$>$
- \item 2004/02/10 acpi and option rom updates
- \item 2003/11/18 initial release
- \end{itemize}
-
-
-
-%
-% 3 What is coreboot
-%
-
-\section{What is coreboot?}
-
+\section{What is Coreboot}
 coreboot aims to replace the normal BIOS found on x86, AMD64, PPC,
 Alpha, and other machines with a Linux kernel that can boot Linux from a cold
 start. The startup code of an average coreboot port is about 500 lines of
@@ -91,1663 +60,555 @@ people with varying backgrounds.  Nowadays a large and growing number of
 Systems can be booted with coreboot, including embedded systems,
 Desktop PCs and Servers.
 
+This document is used to build, modify, and port the CoreBoot code
+base on the AMD platform.
+
+
+\section{Changes}
+
+ \begin{itemize}
+ \item 2013/12/20 Add Git, Gerrit, toolchains building.
+ \item 2009/04/19 replace LinuxBIOS with coreboot
+ \item 2004/06/02 url and language fixes from Ken Fuchs $<$kfuchs@winternet.com$>$
+ \item 2004/02/10 acpi and option rom updates
+ \item 2003/11/18 initial release
+ \end{itemize}
+
 %
-% 4 Build Requirements
+% Build Requirements
 %
 
 \section{Build Requirements}
-To build coreboot for AMD64 from the sources you need a recent Linux
-system for x86 or AMD64. SUSE Linux 8.2 or 9.0 are known to work fine.
-The following toolchain is recommended:
+To build coreboot for AMD64 from the sources you need a recent Linux.
+SUSE Linux 11.2, CentOS release 6.3, Fedora Core 16, Cygwin, FreeBSD,
+NetBSD are known to work fine.
+
+To build the toolchain, you need following host compilers:
 
  \begin{itemize}
- \item GCC 3.3.1
- \item binutils 2.14.90.0.5
- \item Python 2.3
- \item CVS 1.11.6
+ \item GNUtar
+ \item GNUpatch
+ \item GNUmake
+ \item GCC
+ \item binutils
+ \item bison
+ \item flex
+ \item m4
+ \item wget
  \end{itemize}
 
-\textbf{NOTE:} Later versions should also work. Prior versions might lead to problems.
+Besides the tools above, after the toolchains are built, you also need the following
+tools to build the source.
 
-\newpage
+ \begin{itemize}
+ \item git: Get the source code from repository
+ \item libncurses-dev (or ncursesw, ncurses, curses, pdcursesw, pdcurses): for menuconfig
+ \item python: Optional for gdb.
+ \item perl: Optional for gdb.
+ \end{itemize}
 
 %
-% 5 Getting the Sources
+% Getting Coreboot
 %
 
-\section{Getting the Sources}
-
-The latest coreboot sources are available via subversion. The subversion
-repository is maintained at SourceForge.net (the project name is
-\emph{FreeBIOS}).  First you should create a directory for your
-coreboot trees:
-
+\section{Getting Coreboot}
+The latest coreboot sources are available via GIT.
+For users who doesn't need to change and commit the code:
 { \small
 \begin{verbatim}
-$ mkdir coreboot
-$ cd coreboot
+$ git clone http://review.coreboot.org/p/coreboot
 \end{verbatim}
 }
-
-You can get the entire source tree via SVN:
-
+For developers, you need to get a gerrit account which you can register
+at \url{http://review.coreboot.org}. Please refer section ~\ref{sec:gerrit}
 { \small
 \begin{verbatim}
-$ svn co svn://coreboot.org/repos/trunk/coreboot-v2
+$ git clone ssh://<username>@review.coreboot.org:29418/coreboot
+$ git clone http://[<username>:<password>@]review.coreboot.org/coreboot.git
 \end{verbatim}
 }
 
-Once the source tree is checked out, it can be updated with:
-
+Checks out a sub-repository in the 3rdparty directory.
 { \small
 \begin{verbatim}
-% svn update
+$ git submodule update --init --checkout
 \end{verbatim}
 }
 
-For the case your corporate firewall blocks port 3690 (subversion) we set up a
-snapshot site that keeps the last few hundred source code revisions. It
-is available at \url{http://qa.coreboot.org/}.
-Due to major structural enhancements to \hbox{coreboot}, AMD64 support
-is only available in the \texttt{coreboot-v2} tree. This tree reflects (as
-of November 2003) coreboot version 1.1.5 and will lead to coreboot 2.0
-when finished.  Most x86 hardware is currently only supported by the
-coreboot 1.0 tree.
-
-%
-% 6 coreboot configuration overview
-%
-
-\section{coreboot configuration overview}
-To support a large variety of existing hardware coreboot allows for a
-lot of configuration options that can be tweaked in several ways:
-
-\begin{itemize}
-\item
-Firmware image specific configuration options can be set in the image
-configuration file which is usually found in
-\texttt{coreboot-v2/targets/$<$vendor$>$/$<$mainboard$>$/}.  Such
-options are the default amount of output verbosity during bootup, image
-size, use of fallback mechanisms, firmware image size and payloads
-(Linux Kernel, Bootloader...) The default configuration file name is
-\texttt{Config.lb}, but coreboot allows multiple configurations to
-reside in that directory.
-
-\item Mainboard specific configuration options can be set in the
-mainboard configuration file placed in
-\texttt{coreboot-v2/src/mainboard/$<$vendor$>$/$<$mainboard$>$}. The
-mainboard configuration file is always called \texttt{Config.lb}. It
-contains information on the onboard components of the mainboard like
-CPU type, northbridge, southbridge, hypertransport configuration and
-SuperIO configuration.  This configuration file also allows to include
-addon code to hook into the coreboot initialization mechanism at
-basically any point.
-
-\end{itemize}
-
-This document describes different approaches of changing and configuring the
-coreboot source tree when building for AMD64.
-
-%
-% 7 Building coreboot
-%
-
-\section{Building coreboot}
-One of the design goals for building coreboot was to keep object files
-out of the source tree in a separate place. This is mandatory for
-building parallel coreboot images for several distinct mainboards
-and/or platforms. Therefore building coreboot consists of two steps:
-\begin{itemize}
-\item
-creating a build tree which holds all files automatically created by the
-configuration utility and the object files
-\item
-compiling the coreboot code and creating a flashable firmware image.
-\end{itemize}
-
-The first of these two steps is accomplished by the \texttt{buildtarget}
-script found in \texttt{coreboot-v2/targets/}. To build coreboot for
-instance for the AMD Solo Athlon64 mainboard enter:
-
-\begin{verbatim}
-% cd coreboot-v2/targets
-% ./buildtarget amd/solo
-\end{verbatim}
-
-This will create a directory containing a Makefile and other software
-components needed for this build. The directory name is defined in the
-firmware image specific configuration file. In the case of AMD's Solo
-mainboard the default directory resides in
-\texttt{coreboot-v2/targets/amd/solo/solo}. To build the coreboot image, do
-
-\begin{verbatim}
-% cd amd/solo/solo
-% make
-\end{verbatim}
-
-The coreboot image filename is specified in the firmware image specific
-configuration file. The default filename for AMD's Solo mainboard is
-\texttt{solo.rom}.
-
 %
-% 8 Programming coreboot to flash memory
+% Building the toolchain
 %
 
-\section{Programming coreboot to flash memory}
-The image resulting from a coreboot build can be directly programmed to
-a flash device, either using a hardware flash programmer or by using the
-Linux flash driver devbios or mtd. This document assumes that you use a
-hardware flash programmer. If you are interested in doing in-system
-software flash programming, find detailed information:
-
-\begin{itemize}
-\item \url{http://www.openbios.org/development/devbios.html} (/dev/bios)
-\item \url{http://www.linux-mtd.infradead.org/} (Memory Technology Device Subsystem MTD)
-\end{itemize}
-
-\newpage
-
-%
-% 9 coreboot configuration
-%
-
-\section{coreboot configuration}
-The following chapters will cope with configuring coreboot. All
-configuration files share some basic rules
-\begin{itemize}
-\item
-The default configuration file name in coreboot is \texttt{Config.lb}.
-\item
-All variables used in a configuration file have to be declared in this
-file with \texttt{uses VARNAME} before usage.
-\item
-Comments can be added on a new line by using the comment identifier
-\texttt{\#} at the beginning of the line.
-\item
-coreboot distinguishes between statements and options. Statements cause
-the coreboot configuration mechanism to act, whereas options set
-variables that are used by the build scripts or source code.
-\item
-Default configuration values can be set in the mainboard configuration
-files (keyword default)
-\item
-Option overrides to the default configuration can only be specified in
-the build target configuration file
-\texttt{coreboot-v2/targets/$<$vendor$>$/$<$mainboard$>$/Config.lb}
-(keyword option)
-\end{itemize}
-
-\subsection{Common Configuration Statements}
-
-\begin{itemize}
-
-\item \begin{verbatim}uses\end{verbatim}
-
-All local configuration variables have to be declared before they can be
-used. Example:
-\begin{verbatim}
-        uses CONFIG_ROM_IMAGE_SIZE
-\end{verbatim}
-
-\textbf{NOTE:} Only configuration variables known to the configuration
-system can be used in configuration files. coreboot checks
-\texttt{coreboot-v2/src/config/Options.lb} to see whether a configuration
-variable is known.
-
-\item \begin{verbatim}default\end{verbatim}
-
-The \texttt{default} statement is used to set a configuration variable
-with an overridable default value. It is commonly used in mainboard
-configuration files.
-
-Example:
-
-\begin{verbatim}
-        default CONFIG_ROM_IMAGE_SIZE=0x10000
-\end{verbatim}
-
-It is also possible to assign the value of one configuration variable to
-another one, i.e.:
-
-\begin{verbatim}
-        default CONFIG_FALLBACK_SIZE=CONFIG_ROM_SIZE
-\end{verbatim}
-
-Also, simple expressions are allowed:
-
-\begin{verbatim}
-        default CONFIG_FALLBACK_SIZE=(CONFIG_ROM_SIZE -  NORMAL_SIZE)
-\end{verbatim}
-
-If an option contains a string, this string has to be protected with
-quotation marks:
-
-\begin{verbatim}
-        default CC="gcc -m32"
-\end{verbatim}
-
-\item \begin{verbatim}option\end{verbatim}
-
-The \texttt{option} statement basically behaves identically to the
-\texttt{default} statement. But unlike default it can only be used in
-build target configuration files
-(\texttt{coreboot-v2/targets/$<$vendor$>$/$<$mainboard$>$}). The option
-statement allows either to set new options or to override default values
-set with the default statement in a mainboard configuration file.
-Syntax and application are the same as with default.
-
-\end{itemize}
-
-\subsection{Firmware image specific configuration}
-coreboot allows to create different firmware images for the same
-hardware. Such images can differ in the amount of output they produce,
-the payload, the number of subimages they consist of etc.
-
-The firmware image specific configuration file can be found in \\
-\texttt{coreboot-v2/targets/$<$vendor$>$/<mainboard$>$}.
-
-\subsubsection{Firmware image specific keywords}
-In addition to the above described keywords the following statements are
-available in firmware image specific configuration files:
-
-\begin{itemize}
-\item \begin{verbatim}romimage\end{verbatim}
-
-The \texttt{romimage} definition describes a single rom build within the
-final coreboot image. Normally there are two romimage definitions per
-coreboot build: \texttt{normal} and \texttt{fallback}.
-
-Each \texttt{romimage} section needs to specify a mainboard directory and a
-payload. The mainboard directory contains the mainboard specific
-configuration file and source code. It is specified relatively to
-\texttt{coreboot-v2/src/mainboard}. The payload definition is an absolute
-path to a static elf binary (i.e Linux kernel or etherboot)
+\section{Building the toolchain}
+Coreboot recommends and guarantees the toolchain integrated with Coreboot.
+Linux distributions usually modify their compilers in ways incompatible with Coreboot.
 
+{ \small
 \begin{verbatim}
-romimage "normal"
-        option CONFIG_USE_FALLBACK_IMAGE=0
-        option CONFIG_ROM_IMAGE_SIZE=0x10000
-        option COREBOOT_EXTRA_VERSION=".0Normal"
-        mainboard amd/solo
-        payload /suse/stepan/tg3ide_
-        disk.zelf
-end
+$ cd coreboot
+$ make crossgcc
 \end{verbatim}
+}
 
-\item \begin{verbatim}buildrom\end{verbatim}
-
-The \texttt{buildrom} statement is used to determine which of the
-coreboot image builds (created using \texttt{romimage}) are packed
-together to the final coreboot image. It also specifies the order of
-the images and the final image size:
+or
 
+{ \small
 \begin{verbatim}
-        buildrom ./solo.rom CONFIG_ROM_SIZE "normal" "fallback"
+$ cd util/crossgcc
+$ buildgcc
 \end{verbatim}
+}
 
-\end{itemize}
-
-
-\subsubsection{Firmware image configuration options}
-In addition to the definitions described above there are a number of
-commonly used options. Configuration options set in the firmware image
-specific configuration file can override default selections from the
-Mainboard specific configuration.  See above examples about
-option on how to set them.
-
-\begin{itemize}
-
-\item \begin{verbatim}CC\end{verbatim}
-
-Target C Compiler. Default is \texttt{\$(CROSS\_COMPILE)gcc}. Set to
-\texttt{gcc -m32} for compiling AMD64 coreboot images on an AMD64
-machine.
-
-\item \begin{verbatim}CONFIG_CHIP_CONFIGURE \end{verbatim}
-
-Use new \textit{chip\_configure} method for configuring (nonpci)
-devices. Set to \texttt{1} for all AMD64 mainboards.
-
-\item \begin{verbatim}CONFIG_DEFAULT_CONSOLE_LOGLEVEL\end{verbatim}
-
-Console will log at this level unless changed. Default is \texttt{7},
-minimum is \texttt{0}, maximum is \texttt{10}.
+The buildgcc will try to get packages from website. You need to make sure you can
+get access the internet. Or you can get the source.tar.gz and put it in util/crossgcc/tarballs.
 
-\item \begin{verbatim}CONFIG_CONSOLE_SERIAL8250\end{verbatim}
+{ \small
+\textcolor{blue} {Welcome to the} \textcolor{red} {coreboot} \textcolor{blue} {cross toolchain builder v1.23 (September 20th, 2013)}
 
-Log messages to 8250 uart based serial console. Default is \texttt{0}
-(don't log to serial console). This value should be set to \texttt{1}
-for all AMD64 builds.
+Target arch is now i386-elf
 
-\item \begin{verbatim}CONFIG_ROM_SIZE\end{verbatim}
+Will skip GDB ... ok
 
-Size of final ROM image. This option has no default value.
+Downloading tar balls ...
 
-\item \begin{verbatim}CONFIG_FALLBACK_SIZE\end{verbatim}
+ * gmp-5.1.2.tar.bz2 (cached)
 
-Fallback image size. Defaults to \texttt{65536} bytes. \textbf{NOTE:}
-This does not include the fallback payload.
+ * mpfr-3.1.2.tar.bz2 (cached)
 
-\item \begin{verbatim}CONFIG_HAVE_OPTION_TABLE\end{verbatim}
+ * mpc-1.0.1.tar.gz (cached)
 
-Export CMOS option table. Default is \texttt{0}. Set to \texttt{1} if
-your mainboard has CMOS memory and you want to use it to store
-coreboot parameters (Loglevel, serial line speed, ...)
+ * libelf-0.8.13.tar.gz (cached)
 
-\item \begin{verbatim}CONFIG_ROM_PAYLOAD\end{verbatim}
+ * gcc-4.7.3.tar.bz2 (cached)
 
-Boot image is located in ROM (as opposed to \texttt{CONFIG\_IDE\_PAYLOAD}, which
-will boot from an IDE disk)
+ * binutils-2.23.2.tar.bz2 (cached)
 
-\item \begin{verbatim}CONFIG_HAVE_FALLBACK_BOOT\end{verbatim}
+ * acpica-unix-20130626.tar.gz (cached)
 
-Set to \texttt{1} if fallback booting is required. Defaults to
-\texttt{0}.
+Downloaded tar balls ... \textcolor {green}{ok}
 
-\end{itemize}
+Unpacking and patching ...
 
+ * gmp-5.1.2.tar.bz2
 
-The following options should be used within a romimage section:
+ * mpfr-3.1.2.tar.bz2
 
-\begin{itemize}
+ * mpc-1.0.1.tar.gz
 
-\item \begin{verbatim}CONFIG_USE_FALLBACK_IMAGE\end{verbatim}
+ * libelf-0.8.13.tar.gz
 
-Set to \texttt{1} to build a fallback image. Defaults to \texttt{0}
+ * gcc-4.7.3.tar.bz2
 
-\item \begin{verbatim}CONFIG_ROM_IMAGE_SIZE\end{verbatim}
+ * binutils-2.23.2.tar.bz2
 
-Default image size. Defaults to \texttt{65535} bytes.
+   o binutils-2.23.2\_arv7a.patch
 
-\item \begin{verbatim}COREBOOT_EXTRA_VERSION\end{verbatim}
+   o binutils-2.23.2\_no-bfd-doc.patch
 
-coreboot extra version. This option has an empty string as default. Set
-to any string to add an extra version string to your coreboot build.
+ * acpica-unix-20130626.tar.gz
 
-\end{itemize}
-
-\newpage
+Unpacked and patched ... \textcolor {green}{ok}
 
-\subsection{Mainboard specific configuration}
+Building GMP 5.1.2 ... \textcolor {green}{ok}
 
-Mainboard specific configuration files describe the onboard
-mainboard components, i.e. bridges, number and type of CPUs. They also
-contain rules for building the low level start code which is translated
-using romcc and/or the GNU assembler.  This code enables caches and
-registers, early mtrr settings, fallback mechanisms, dram init and
-possibly more.
+Building MPFR 3.1.2 ... \textcolor {green}{ok}
 
-\textbf{NOTE:} The \texttt{option} keyword can not be used in mainboard
-specific configuration files.  Options shall instead be set using the
-\texttt{default} keyword so that they can be overridden by the image
-specific configuration files if needed.
+Building MPC 1.0.1 ... \textcolor {green}{ok}
 
-\subsubsection{Mainboard specific keywords}
+Building libelf 0.8.13 ... \textcolor {green}{ok}
 
-The following statements are used in mainboard specific configuration
-files:
+Building binutils 2.23.2 ... \textcolor {green}{ok}
 
-\begin{itemize}
-\item \begin{verbatim}arch\end{verbatim}
+Building GCC 4.7.3 ...  ok
 
-Sets the CPU architecture. This should be \texttt{i386} for AMD64 boards.\\
-Example:
+Skipping Expat (Python scripting not enabled)
 
-\begin{verbatim}
-        arch i386 end
-\end{verbatim}
+Skipping Python (Python scripting not enabled)
 
-\item \begin{verbatim}cpu\end{verbatim}
+Skipping GDB (GDB support not enabled)
 
-The cpu statement is needed once per possibly available CPU. In a
-one-node system, write:
+Building IASL 20130626 ... \textcolor {green}{ok}
 
-\begin{verbatim}
-        cpu k8 "cpu0" end
-\end{verbatim}
+Cleaning up... \textcolor {green}{ok}
 
-\item \begin{verbatim}driver\end{verbatim}
+\textcolor {green}{You can now run your i386-elf cross toolchain from /home/baozheng/x86/coreboot-gerrit/util/crossgcc/xgcc.}
+}
+If you are lucky, you can get toolchains located in util/crossgcc/xgcc.
 
-The \texttt{driver} keyword adds an object file to the driver section of a
-coreboot image.  This means it can be used by the PCI device
-initialization code. Example:
+%
+% Build Coreboot
+%
 
+\section{Building Coreboot}
+\subsection{Build main module of Coreboot}
+{ \small
 \begin{verbatim}
-        driver mainboard.o
+$ cd coreboot
+$ make menuconfig
+.config - coreboot v4.0-4895-gc5025a4-dirty Configuration
++------------------------ coreboot Configuration -------------------------+
+|  Arrow keys navigate the menu.  <Enter> selects submenus --->.          |
+|  Highlighted letters are hotkeys.  Pressing <Y> includes, <N> excludes, |
+|  <M> modularizes features.  Press <Esc><Esc> to exit, <?> for Help, </> |
+|  for Search.  Legend: [*] built-in  [ ] excluded  <M> module  < >       |
+| +---------------------------------------------------------------------+ |
+| |        General setup  --->                                          | |
+| |        Mainboard  --->                                              | |
+| |        Architecture (x86)  --->                                     | |
+| |        Chipset  --->                                                | |
+| |        Devices  --->                                                | |
+| |        VGA BIOS  --->                                               | |
+| |        Display  --->                                                | |
+| |        PXE ROM  --->                                                | |
+| |        Generic Drivers  --->                                        | |
+| |        Console  --->                                                | |
+| |    [ ] Relocatable Modules                                          | |
+| |        System tables  --->                                          | |
+| |        Payload  --->                                                | |
+| |        Debugging  --->                                              | |
+| |    ---                                                              | |
+| +----v(+)-------------------------------------------------------------+ |
++-------------------------------------------------------------------------+
+|                    <Select>    < Exit >    < Help >                     |
++-------------------------------------------------------------------------
 \end{verbatim}
+}
+Select Mainboard -$>$ Mainboard Vendor -$>$ AMD
+                 -$>$ Mainboard Model  -$>$ Olive Hill
 
-\item \begin{verbatim}object\end{verbatim}
-
-The \texttt{object} keyword adds an object file to the coreboot image.
-Per default the object file will be compiled from a \texttt{.c} file
-with the same name. Symbols defined in such an object file can be used
-in other object files and drivers. Example:
+Then save, exit and run make.
 
+{ \small
 \begin{verbatim}
-        object reset.o
+$ make
 \end{verbatim}
+}
+The built image, coreboot.rom, is located at folder build.
 
-\item \begin{verbatim}makerule\end{verbatim}
+\section{Programming coreboot to flash memory}
+The image resulting from a coreboot build can be directly programmed to
+a flash device, either using an external flash programmers, e.g., Dediprog SF100, or by using the
+Linux flash utility, flashrom.
 
-This keyword can be used to extend the existing file creation rules
-during the build process. This is useful if external utilities have to
-be used for the build. coreboot on AMD64 uses romcc for it's early
-startup code placed in auto.c.
 
-To tell the configuration mechanism how to build \texttt{romcc} files,
-do:
+\subsection{Add modules and payload}
 
+\subsubsection{VGA BIOS}
+There is a big Chance that you need to get a VGA BIOS.
+{ \small
 \begin{verbatim}
-makerule ./auto.E
-        depends "$(CONFIG_MAINBOARD)/auto.c option_table.h ./romcc"
-        action "./romcc -E -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) \
-		$(CONFIG_MAINBOARD)/auto.c -o $@"
-end
-makerule ./auto.inc
-        depends "$(CONFIG_MAINBOARD)/auto.c option_table.h ./romcc"
-        action "./romcc    -mcpu=k8 -O2 -I$(TOP)/src -I. $(CPPFLAGS) \
-                $(CONFIG_MAINBOARD)/auto.c -o $@"
-end
+.config - coreboot v4.0 Configuration
+------------------------------------------------------------------------------
++-------------------------------- VGA BIOS --------------------------------+
+|  Arrow keys navigate the menu.  <Enter> selects submenus --->.           |
+|  Highlighted letters are hotkeys.  Pressing <Y> includes, <N> excludes,  |
+|  <M> modularizes features.  Press <Esc><Esc> to exit, <?> for Help, </>  |
+|  for Search.  Legend: [*] built-in  [ ] excluded  <M> module  < > module |
+| +----------------------------------------------------------------------+ |
+| |    [*] Add a VGA BIOS image                                          | |
+| |    (vgabios.bin) VGA BIOS path and filename                          | |
+| |    (1002,1306) VGA device PCI IDs                                    | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| +----------------------------------------------------------------------+ |
++--------------------------------------------------------------------------+
+|                     <Select>    < Exit >    < Help >                     |
++--------------------------------------------------------------------------+
 \end{verbatim}
+}
+Select VGA BIOS. ``The VGA device PCI IDs'' should be the same as your device. Get the
+Option ROM from Vendor's website.
 
-Each \texttt{makerule} section contains file dependencies (using the
-texttt{depends} keyword) and an action that is taken when the dependencies
-are satisfied (using the \texttt{action} keyword).
-
-\item \begin{verbatim}mainboardinit\end{verbatim}
-
-With the mainboardinit keyword it's possible to include assembler code
-directly into the coreboot image. This is used for early infrastructure
-initialization, i.e. to switch to protected mode. Example:
+\subsubsection{Payload}
+coreboot in itself is "only" minimal code for initializing a mainboard
+with peripherals. After the initialization, it jumps to a payload.
 
+Currently, SeaBIOS is the most widely used payload. The best way to integrate SeaBIOS
+is setting it in menuconfig.
+{ \small
 \begin{verbatim}
-        mainboardinit cpu/i386/entry16.inc
-\end{verbatim}
-
-\item \begin{verbatim}ldscript\end{verbatim}
-
-The GNU linker ld is used to link object files together to a coreboot
-ROM image.
-
-Since it is a lot more comfortable and flexible to use the GNU linker
-with linker scripts (ldscripts) than to create complex command line
-calls, coreboot features including linker scripts to control image
-creation. Example:
-
++------------------------------- Payload ---------------------------------+
+|  Arrow keys navigate the menu.  <Enter> selects submenus --->.           |
+|  Highlighted letters are hotkeys.  Pressing <Y> includes, <N> excludes,  |
+|  <M> modularizes features.  Press <Esc><Esc> to exit, <?> for Help, </>  |
+|  for Search.  Legend: [*] built-in  [ ] excluded  <M> module  < > module |
+| +----------------------------------------------------------------------+ |
+| |        Add a payload (SeaBIOS)  --->                                 | |
+| |        SeaBIOS version (1.7.2.1)  --->                               | |
+| |    [*] Use LZMA compression for payloads (NEW)                       | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| |                                                                      | |
+| +----------------------------------------------------------------------+ |
++--------------------------------------------------------------------------+
+|                     <Select>    < Exit >    < Help >                     |
++--------------------------------------------------------------------------+
+\end{verbatim}
+The script in Makefile will automatically checkout, config, build the SeaBIOS source,
+and integrat the binary into the final image.
+
+%
+% Working with Git
+%
+
+\section{Working with Git}
+\subsection{Configuration of Git}
+Inside the checkout you should install a commit-msg hook that adds a
+Change-Id into commit messages, which uniquely identifies the logical
+change in Gerrit even across multiple iterations of the commit. The
+hook only needs to be installed once per clone, and installation can
+be done with:
+{ \small
 \begin{verbatim}
-        ldscript /cpu/i386/entry16.lds
+$ cd coreboot
+$ cp ./util/gitconfig/* .git/hooks
 \end{verbatim}
-
-
-\item \begin{verbatim}dir\end{verbatim}
-
-coreboot reuses as much code between the different ports as possible.
-To achieve this, commonly used code can be stored in a separate
-directory. For a new mainboard, it is enough to know that the code in
-that directory can be used as is.
-
-coreboot will also read a \texttt{Config.lb} file stored in that
-directory. This happens with:
-
+}
+configure your name and email in git.
+{ \small
 \begin{verbatim}
-        dir /pc80
+$ git config --global user.name "Your Name Comes Here"
+$ git config --global user.email your.email@example.com'
 \end{verbatim}
+}
+The name~\ref{user name} and email~\ref{Contact Information} should be the same the settings in gerrit.
+Otherwise you can not push you code to community.
 
-
-\item \begin{verbatim}config\end{verbatim}
-
-This keyword is needed by the new chip configuration scheme. Should be
-used as:
-
+Then run the following command once, to tell git that by default you
+want to submit all commits in the currently checked-out branch for
+review on gerrit:
+{ \small
 \begin{verbatim}
-        config chip.h
+$ git config remote.origin.push HEAD:refs/for/master
 \end{verbatim}
+}
 
-\item \begin{verbatim}register\end{verbatim}
-The \texttt{register} keyword can occur in any section, passing
-additional \\
-parameters to the code handling the associated device.
-Example:
-
+The above configurations for git has been integrated into Makefile. You can run
+{ \small
 \begin{verbatim}
-        register "com1" = "{1, 0, 0x3f8, 4}"
+$ make gitconfig
 \end{verbatim}
+}
 
-\item \begin{verbatim}northbridge\end{verbatim}
-
-The \texttt{northbridge} keyword describes a system northbridge. Some
-systems, like AMD64, can have more than one northbridge, i.e. one per
-CPU node. Each northbridge is described by the path to the northbridge
-code in coreboot (relative to \texttt{coreboot-v2/src/northbridge}), i.e.
-\texttt{amd/amdk8} and a unique name (i.e \texttt{mc0}) \\
-Example:
+\subsection{Work flow}
 
+It is recommended that you make a new branch when you start to work, not pushing changes to master.
+{ \small
 \begin{verbatim}
-        northbridge amd/amdk8 "mc0"
-                [..]
-        end
+$ git checkout master -b mybranch
 \end{verbatim}
-
-\item \begin{verbatim}southbridge\end{verbatim}
-
-To simplify the handling of bus bridges in a coreboot system, all
-bridges available in a system that are not northbridges (i.e AGP, IO,
-PCIX) are seen as southbridges.
-
-Since from the CPUs point of view any southbridge is connected via the
-northbridge, a southbridge section is declared within the northbridge
-section of the north bridge it is attached to.
-
-Like the northbridge, any other bridge is described by the path to it's
-driver code, and a unique name. If the described bridge is a
-hypertransport device, the northbridge's hypertransport link it connects
-to can be specified using the \texttt{link} keyword. Example:
-
+}
+After you have done your changes, run:
+{ \small
 \begin{verbatim}
-northbridge amd/amdk8 "mc0"
-        [..]
-        southbridge amd/amd8111 "amd8111" link 0
-                [..]
-        end
-        [..]
-end
+$ git add file_need_to_submit.c
+$ git commit -m "my first change."
 \end{verbatim}
+}
 
-\item \begin{verbatim}pci\end{verbatim}
-
-The \texttt{pci} keyword can only occur within a \texttt{northbridge} or
-\texttt{southbridge} section. It is used to describe the PCI devices
-that are provided by the bridge.  Generally all bridge sections have a
-couple of \texttt{pci} keywords.
-
-The first occurrence of the \texttt{pci} keyword tells coreboot where
-the bridge devices start, relative to the PCI configuration space used
-by the bridge. The following occurences of the \texttt{pci} keyword
-describe the provided devices.
-
-Adding the option \texttt{on} or \texttt{off} to a PCI device will
-enable or disable this device. This feature can be used if some bridge
-devices are not wired to hardware outputs and thus are not used.
+% Does anyone have a better word to describe the phylosophy of spliting changes to patches?
+You need to realize that the changes you have made should be well devided into
+several commits. Each of them has one and only one meaning. You could use git rebase -i to
+split, squash, remove, rewrite you comment.
 
-Example:
+Here is an example of a well-formatted commit message:
 
+{ \small
 \begin{verbatim}
-northbridge amd/amdk8 "mc1"
-        pci 0:19.0
-        pci 0:19.0
-        pci 0:19.0
-        pci 0:19.1
-        pci 0:19.2
-        pci 0:19.3
-end
-\end{verbatim}
+examplecomponent: Refactor duplicated setup into a function
 
-or
+Setting up the demo device correctly requires the exact same register
+values to be written into each of the PCI device functions. Moving the
+writes into a function allows also otherexamplecomponent to use them.
 
-\begin{verbatim}
-southbridge amd/amd8111 "amd8111" link 0
-        pci 0:0.0
-        pci 0:1.0 on
-        pci 0:1.1 on
-        pci 0:1.2 on
-        pci 0:1.3 on
-        pci 0:1.5 off
-        pci 0:1.6 off
-        pci 1:0.0 on
-        pci 1:0.1 on
-        pci 1:0.2 on
-        pci 1:1.0 off
-        [..]
-end
+Signed-off-by: Joe Hacker <joe@hacker.email>
 \end{verbatim}
+}
 
-\item \begin{verbatim}superio\end{verbatim}
-
-SuperIO devices are basically handled like brigdes. They are taking
-their driver code from \texttt{coreboot-v2/src/superio/}. They don't
-provide a PCI compatible configuration interface, but instead are ISA
-PnP devices. Normally they are connected to a southbridge. If this is
-the case, the \texttt{superio} section will be a subsection of the
-\texttt{southbridge} section of the southbridge it is connected to.
-Example:
-
+Then you can push the code.
+{ \small
 \begin{verbatim}
-superio nsc/pc87360 link 1
-        pnp 2e.0
-        pnp 2e.1
-        pnp 2e.2
-        pnp 2e.3
-        pnp 2e.4
-        pnp 2e.5
-        pnp 2e.6
-        pnp 2e.7
-        pnp 2e.8
-        pnp 2e.9
-        pnp 2e.a
-        register "com1" = "{1, 0, 0x3f8, 4}"
-        register "lpt" = "{1}"
-end
+$ git push
 \end{verbatim}
+}
 
-\end{itemize}
-
-\newpage
-
-\subsubsection{Mainboard specific configuration options}
-
-The following options are commonly used in mainboard specific
-configuration files.
-
-They should be set using the \texttt{default} keyword:
-
-\begin{itemize}
-
-\item \begin{verbatim}CONFIG_HAVE_HARD_RESET\end{verbatim}
-
-If set to \texttt{1}, this option defines that there is a hard reset
-function for this mainboard.  This option is not defined per default.
-
-\item \begin{verbatim}CONFIG_HAVE_PIRQ_TABLE\end{verbatim}
-
-If set to \texttt{1}, this option defines that there is an IRQ Table for
-this mainboard. This option is not defined per default.
-
-\item \begin{verbatim}CONFIG_IRQ_SLOT_COUNT\end{verbatim}
-
-Number of IRQ slots. This option is not defined per default.
-
-\item \begin{verbatim}CONFIG_HAVE_MP_TABLE\end{verbatim}
-
-Define this option to build an MP table (v1.4). The default is not to
-build an MP table.
-
-\item \begin{verbatim}CONFIG_HAVE_OPTION_TABLE\end{verbatim}
-
-Define this option to export a CMOS option table. The default is not to
-export a CMOS option table.
-
-\item \begin{verbatim}CONFIG_SMP\end{verbatim}
-
-Set this option to \texttt{1} if the mainboard supports symmetric
-multiprocessing (SMP). This option defaults to \texttt{0} (no SMP).
-
-\item \begin{verbatim}CONFIG_MAX_CPUS\end{verbatim}
-
-If \begin{verbatim}CONFIG_SMP\end{verbatim} is set, this option defines
-the maximum number of CPUs (i.e. the number of CPU sockets) in the
-system. Defaults to \texttt{1}.
-
-\item \begin{verbatim}CONFIG_IOAPIC\end{verbatim}
-
-Set this option to \texttt{1} to enable IOAPIC support. This is
-mandatory if you want to boot a 64bit Linux kernel on an AMD64 system.
-
-\item \begin{verbatim}CONFIG_STACK_SIZE\end{verbatim}
-
-coreboot stack size. The size of the function call stack defaults to
-\texttt{0x2000} (8k).
-
-\item \begin{verbatim}CONFIG_HEAP_SIZE\end{verbatim}
-
-coreboot heap size. The heap is used when coreboot allocates memory
-with malloc(). The default heap size is \texttt{0x2000}, but AMD64 boards
-generally set it to \texttt{0x4000} (16k)
-
-\item \begin{verbatim}CONFIG_XIP_ROM_BASE\end{verbatim}
-
-Start address of area to cache during coreboot execution directly from
-ROM.
-
-\item \begin{verbatim}CONFIG_XIP_ROM_SIZE\end{verbatim}
-
-Size of area to cache during coreboot execution directly from ROM
-
-\item \begin{verbatim}CONFIG_COMPRESS\end{verbatim}
+You can go to the ~\ref{sec:gerrit} gerrit to see if your changes is successfully pushed.
 
-Set this option to \texttt{1} for a compressed image. If set to
-\texttt{0}, the image is bigger but will start slightly faster (since no
-decompression is needed).
+Often it might happen that the patch you sent for approval is not good
+enough from the first attempt. Gerrit and git make it easy to track
+patch evolution during the review process until patches meet our
+quality standards and are ready for approval.
 
-\end{itemize}
+You can easily modify a patch sent to gerrit by you or even by someone
+else. Just apply it locally using one of the possible ways to do it,
+make a new local commit that fixes the issues reported by the
+reviewers, then rebase the change by preserving the same Change-ID. We
+recommend you to use the git rebase command in interactive mode,
 
-
-\newpage
+Once your patch gets a +2 comment, your patch can be merged (cherry-pick, actually) to origin/master.
 
 %
-% 10. Tweaking the source code
+% Working with Gerrit
 %
 
-\section{Tweaking the source code}
-Besides configuring the existing code it is sometimes necessary or
-desirable to tweak certain parts of coreboot by direct changes to the
-code. This chapter covers some possible enhancements and changes that
-are needed when porting coreboot to a new mainboard or just come
-handy now and then.
-
-\subsection{Hypertransport configuration}
-Before coreboot is able to activate all CPUs and detect bridges
-attached to these CPUs (and thus, see all devices attached to the
-system) it has to initialize the coherent hypertransport devices.
-
-The current algorithms to do coherent hypertransport initialization are
-not fully, automatically evaluating the hypertransport chain graph.
-Therefore the code needs to be adapted when porting coreboot to a new
-AMD64 mainboard. An example arrangement of hypertransport devices
-looks like this:
-
-\begin{figure}[htb]
-\centering
-\includegraphics[scale=1.0]{hypertransport.pdf}
-\caption{Example: Hypertransport Link Connections}
-\label{fix:hypertransport}
-\end{figure}
-
-Each hypertransport device has one to three hypertransport links that
-are used for device interconnection. These links are called LDT$[$012$]$, or
-accordingly UP, ACROSS, DOWN.  Communication between the hypertransport
-devices can be freely routed, honoring the physical wiring. Teaching the
-coherent hypertransport initialization algorithm this wiring happens in
-two steps.
-
-\newpage
-
-\begin{enumerate}
-\item Setting outgoing connections
-The algorithm needs to know which outgoing port of a CPU node is
-connected to the directly succeeding node. This is done in
-\texttt{coreboot-v2/src/mainboard/$<$vendor$>$/$<$mainboard$>$/auto.c}
-with a number of preprocessor defines (one define for two-node systems,
-three defines for four-node systems).
-
-The ports in question are flagged with a circle in the graph for
-illustration. For the example graph above (all outgoing connections are
-realized using LDT1/ACROSS) the defines are:
-
-\begin{verbatim}
-#define CONNECTION_0_1 ACROSS
-#define CONNECTION_0_2 ACROSS
-#define CONNECTION_1_3 ACROSS
-\end{verbatim}
-
-\item Describing routing information between CPUs.
-
-There are basically three different message types for hypertransport
-communication:
-\begin{enumerate}
-\item request packages
-\item response packages
-\item broadcast packages
-\end{enumerate}
-
-These three message types are routed using different hypertransport
-ports. The routing information is written to the AMD K8 routing table.
-In an Nnode system this routing table consists of 3*N*N entries , one
-for each message type and for each possible CPU --> CPU communication. For
-simplicity coreboot keeps the 3 routing entries for each CPU --> CPU
-communication in one machine word.  The routing table of each node looks
-like this:
-
-\begin{verbatim}
-/* Routing Table for Node i
- *
- * F0: 0x40, 0x44, 0x48, 0x4c, 0x50, 0x54, 0x58, 0x5c
- * i: 0, 1, 2, 3, 4, 5, 6, 7
- *
- * [ 0: 3] Request Route
- * [0] Route to this node
- * [1] Route to Link 0
- * [2] Route to Link 1
- * [3] Route to Link 2
- * [11: 8] Response Route
- * [0] Route to this node
- * [1] Route to Link 0
- * [2] Route to Link 1
- * [3] Route to Link 2
- * [19:16] Broadcast route
- * [0] Route to this node
- * [1] Route to Link 0
- * [2] Route to Link 1
- * [3] Route to Link 2
- */
-\end{verbatim}
-
-The routing table is passed to the coherent hypertransport
-initialization algorithm by defining a function called
-\texttt{generate\_row()} in \texttt{auto.c}:
+\section{Working with Gerrit}
+\label{sec:gerrit}
+If you are a coreboot user, not planning to contribute, you can skip this section.
+\subsection{Get gerrit account}
+You need to get an OpenID first. Currently Google account give you an OpenID. It means, if you have a gmail account, you have an OpenID. You can try to signed in.
+click \url{http://review.coreboot.org}
 
+%\includegraphics[width=6.00in,height=1.00in]{gerrit_signin.png}
+{ \small
 \begin{verbatim}
-static unsigned int generate_row
-                (uint8_t node, uint8_t row, uint8_t maxnodes)
++-----------------------------------------------------------+
+|All    Projects  Documentation           Register  Sign In |
+|Open Merged   Abandoned                                    |
+|Search for status:open                                     |
++-----------------------------------------------------------+
+|Subject      Status   Owner  Project  Branch Updated CR V  |
+|cpu: Rename..      Alexandru coreboot master 1:20 PM +1    |
+|cpu: Only a..      Alexandru coreboot master 1:17 PM    X  |
+|arch/x86: D..      Alexandru coreboot master 1:09 PM       |
+|                                                           |
+|                                                  Next ->  |
+|Press '?' to view keyboard shortcuts | Powered by Gerrit   |
++-----------------------------------------------------------+
 \end{verbatim}
-
-This function is trivial if there is only one CPU in the system, since
-no routing has to be done:
-
-\begin{verbatim}
-static unsigned int generate_row
-                (uint8_t node, uint8_t row, uint8_t maxnodes)
-{
-        return 0x00010101; /* default row entry */
 }
-\end{verbatim}
+Click ``Sign In'', You will get
 
-On a two-node system things look slightly more complicated. Since the
-coherent hypertransport initialization algorithm works by consecutively
-enabling CPUs, it contains routing information for driving the system
-with one node and two nodes:
-
-\begin{verbatim}
-static unsigned int generate_row
-                (uint8_t node, uint8_t row, uint8_t maxnodes)
-{
-        uint32_t ret=0x00010101; /* default row entry */
-        static const unsigned int rows_2p[2][2] = {
-                { 0x00050101, 0x00010404 },
-                { 0x00010404, 0x00050101 }
-        };
-        if(maxnodes>2) maxnodes=2;
-        if (!(node>=maxnodes || row>=maxnodes)) {
-                ret=rows_2p[node][row];
-        }
-        return ret;
-}
-\end{verbatim}
-
-Systems with four nodes have to contain routing information for one, two
-and four-node setups:
-
-\begin{verbatim}
-static unsigned int generate_row
-                (uint8_t node, uint8_t row, uint8_t maxnodes)
-{
-        uint32_t ret=0x00010101; /* default row entry */
-        static const unsigned int rows_2p[2][2] = {
-                { 0x00030101, 0x00010202 },
-                { 0x00010202, 0x00030101 }
-        };
-        static const unsigned int rows_4p[4][4] = {
-                { 0x00070101, 0x00010202, 0x00030404, 0x00010204 },
-                { 0x00010202, 0x000b0101, 0x00010208, 0x00030808 },
-                { 0x00030808, 0x00010208, 0x000b0101, 0x00010202 },
-                { 0x00010204, 0x00030404, 0x00010202, 0x00070101 }
-        };
-        if (!(node>=maxnodes || row>=maxnodes)) {
-                if (maxnodes==2)
-                        ret=rows_2p[node][row];
-                if (maxnodes==4)
-                        ret=rows_4p[node][row];
-        }
-        return ret;
-}
-\end{verbatim}
-\end{enumerate}
+%\includegraphics[width=6.00in,height=4.00in]{openid.png}
 
-\subsection{DRAM configuration}
-Setting up the RAM controller(s) is probably the most complex part of
-coreboot.  Basically coreboot serially initializes all RAM controllers
-in the system, using SPDROM (serial presence detect) data to set
-timings, size and other properties.  The SPD data is usually read
-utilizing the I2C SMBUS interface of the southbridge.
-
-There is one central data structure that describes the RAM controllers
-available on an AMD64 system and the associated devices:
-
-\begin{verbatim}
-struct mem_controller {
-        unsigned node_id;
-        device_t f0, f1, f2, f3;
-        uint8_t channel0[4];
-        uint8_t channel1[4];
-};
-\end{verbatim}
-
-Available mainboard implementations and CPUs create the need to add
-special setup code to RAM initialization in a number of places.
-coreboot provides hooks to easily add code in these places without
-having to change the generic code.  Whether these hooks have to be used
-depends on the mainboard design. In many cases the functions executed
-by the hooks just carry out trivial default settings or they are even
-empty.
-
-Some mainboard/CPU combinations need to trigger an additional memory
-controller reset before the memory can be initialized properly. This is,
-for example, used to get memory working on preC stepping AMD64
-processors. coreboot provides two hooks for triggering onboard memory
-reset logic:
-
-\begin{itemize}
-\item \begin{verbatim}static void memreset_setup(void)\end{verbatim}
-\item \begin{verbatim}static void memreset(int controllers, const struct
-		mem_controller *ctrl)\end{verbatim}
-\end{itemize}
-
-Some mainboards utilize an SMBUS hub or possibly other mechanisms to
-allow using a large number of SPDROMs and thus ram sockets. The result
-is that only the SPDROM information of one cpu node is visible at a
-time. The following function, defined in \texttt{auto.c}, is called every time
-before a memory controller is initialized and gets the memory controller
-information of the next controller as a parameter:
+You will be redirected to Google to get logging in.
 
+% \includegraphics[width=6.00in,height=1.50in]{login.png}
+{ \small
 \begin{verbatim}
-static inline void activate_spd_rom (const struct mem_controller *ctrl)
-\end{verbatim}
+Sign In to Gerrit Code Review at review.coreboot.org
++--------------------------------------------------+
++--------------------------------------------------+
+[] Remember me
+Sign In Cancel
+Sign in with a Google Account
+Sign in with a Yahoo! ID
+What is OpenID?
 
-The way SMBUS hub information is coded into the \texttt{mem\_controller}
-structure is mainboard implementation specific and not
-described here.  See \texttt{coreboot-v2/src/mainboard/amd/quartet/auto.c}
-for an example.
+OpenID provides secure single-sign-on, without revealing your passwords to this website.
 
-coreboot folks have agreed on SPD data being the central information
-source for RAM specific information. But not all mainboards/RAM
-modules feature a physical SPD ROM. To still allow an easy to use SPD
-driven setup, there is a hook that abstracts reading the SPD ROM
-ingredients that are used by the memory initialization mechanism:
+There are many OpenID providers available. You may already be member of one!
 
-\begin{verbatim}
-static inline int spd_read_byte(unsigned device, unsigned address)
+Get OpenID
 \end{verbatim}
-
-This function, defined in \texttt{auto.c}, directly maps it's calls to
-\texttt{smbus\_read\_byte()} calls if SPD ROM information is read via
-the I2C SMBUS:
-
-\begin{verbatim}
-static inline int spd_read_byte(unsigned device, unsigned address)
-{
-        return smbus_read_byte(device & 0xff, address);
 }
-\end{verbatim}
-
-If there is no SPD ROM available in the system design, this function
-keeps an array of SPD ROM information hard coded per logical RAM module.
-It returns the faked' SPD ROM information using device and address
-as indices to this array.
-
-
-\subsection {IRQ Tables}
-
-Mainboards that provide an IRQ table should have the following two
-variables set in their \texttt{Config.lb} file:
-
-\begin{verbatim}
-default CONFIG_HAVE_PIRQ_TABLE=1
-default CONFIG_IRQ_SLOT_COUNT=7
-\end{verbatim}
-
-This will make coreboot look for the file \\
-\texttt{coreboot-v2/src/mainboard/<vendor>/<mainboard>/irq\_tables.c} which
-contains the source code definition of the IRQ table. coreboot corrects
-small inconsistencies in the IRQ table during startup (checksum and
-number of entries), but it is not yet writing IRQ tables in a completely
-dynamic way.
-
-\textbf{NOTE:} To get Linux to understand and actually use the IRQ
-table, it is not always a good idea to specify the vendor and device id
-of the actually present interrupt router device. Linux 2.4 for example
-does not know about the interrupt router of the AMD8111 southbridge. In
-such cases it is advised to choose the vendor/device id of a compatible
-device that is supported by the Linux kernel. In case of the AMD8111
-interrupt router it is advised to specify the AMD768/Opus interrupt
-controller instead (vendor id=\texttt{0x1022}, device id=\texttt{0x7443})
-
-\subsection {MP Tables}
-
-coreboot contains code to create MP tables conforming the
-Multiprocessor Specification V1.4. To include an MP Table in a coreboot
-image, the following configuration variables have to be set (in the
-mainboard specific configuration file
-\texttt{coreboot-v2/src/mainboard/<vendor><mainboard>/Config.lb}):
-
-\begin{verbatim}
-default CONFIG_SMP=1
-default CONFIG_MAX_CPUS=1 # 2,4,..
-default CONFIG_HAVE_MP_TABLE=1
-\end{verbatim}
-
-coreboot will then look for a function for setting up the MP table in
-the file \texttt{coreboot-v2/src/mainboard<vendor>/<mainboard>/mptable.c}:
 
-\begin{verbatim}
-void *smp_write_config_table(void *v, unsigned long * processor_map)
-\end{verbatim}
-
-MP Table generation is still somewhat static, i.e. changing the bus
-numbering will force
-you to adopt the code in mptable.c. This is subject to change in future
-revisions.
-
-\subsection {ACPI Tables}
-
-There is initial ACPI support in coreboot now. Currently the only gain with
-this is the ability to use HPET timers in Linux. To achieve this, there is a
-framework that can generate the following tables:
-\begin{itemize}
-\item RSDP
-\item RSDT
-\item MADT
-\item HPET
-\end{itemize}
-
-To enable ACPI in your coreboot build, add the following lines to your
-configuration files:
-\begin{verbatim}
-uses CONFIG_HAVE_ACPI_TABLES
-[..]
-option CONFIG_HAVE_ACPI_TABLES=1
-\end{verbatim}
-
-To keep Linux doing it's pci ressource allocation based on IRQ tables and MP
-tables, you have to specify the kernel parameter \texttt{pci=noacpi} otherwise
-your PCI devices won't get interrupts.
-It's likely that more ACPI support will follow, when there is need for certain
-features.
-
-\subsection{POST}
-coreboot has three different methods of handling POST codes. They can
-be triggered using configuration file options.
-\begin{itemize}
-\item
-\emph{Ignore POST completely}. No early code debugging is possible with
-this setting.  Set the configuration variable \texttt{NO\_POST} to
-\texttt{1} to switch off all POST handling in coreboot.
-\item
-\emph{Normal IO port 80 POST}. This is the default behavior of
-coreboot. No configuration variables have to be set. To be able to see
-port 80 POST output, you need a POST expansion card for ISA or PCI. Port
-80 POST allows simple debugging without any other output method
-available (serial interface or VGA display)
-\item
-\emph{Serial POST}.
-This option allows to push POST messages to the serial interface instead
-of using IO ports. \textbf{NOTE:} The serial interface has to be
-initialized before serial POST can work. To use serial POST, set the
-configuration variable \texttt{CONFIG\_SERIAL\_POST} to the value 1.
-\end{itemize}
+\subsection{Configure account}
+Click the dropdown button near the user name and click ``Settings''
 
+% \includegraphics[width=6.00in,height=4.00in]{settings}
+% \epsfig{figure=keystroke_left}
+% \epstopdf {file=settings.eps}
+% \epsfig{file=settings.eps}
 
-\subsection{HDT Debugging}
-If you are debugging your coreboot code with a Hardware Debug Tool
-(HDT), you can find the source code line for a given physical EIP
-address as follows: Look the address up in the file linuxbios.map. Then
-search the label Lxx in the file auto.inc created by romcc. The original
-source code file and line number is mentioned in auto.inc.
-
-
-\subsection{Device Drivers}
-With only a few data structures coreboot features a simple but flexible
-device driver interface. This interface is not intended for autonomously
-driving the devices but to initialize all system components so that they
-can be used by the booted operating system.
-
-Since nowadays most systems are PCI centric, the data structures used
-are tuned towards (onboard and expansion bus) PCI devices. Each driver
-consists of at least two structures.
-
-The \texttt{pci\_driver} structure maps PCI vendor/device id pairs to a
-second structure that describes a set of functions that together
-initialize and operate the device:
-
-\begin{verbatim}
-    static void adaptec_scsi_init(struct device *dev)
-    {
-            [..]
-    }
-    static struct device_operations lsi_scsi_ops = {
-            .read_resources = pci_dev_read_resources,
-            .set_resources = pci_dev_set_resources,
-            .enable_resources = pci_dev_enable_resources,
-            .init = lsi_scsi_init,
-            .scan_bus = 0,
-    };
-    static const struct pci_driver lsi_scsi_driver __pci_driver = {
-            .ops = &lsi_scsi_ops,
-            .vendor = 0xXXXX,
-            .device = 0xXXXX,
-    };
-\end{verbatim}
-
-By separating the two structures above, M:N relations between compatible
-devices and drivers can be described. The driver source code containing
-above data structures and code have to be added to a coreboot image
-using the driver keyword in the mainboard specific configuration file \\
-\texttt{coreboot-v2/src/mainboard/<vendor>/<mainboard>/Config.lb}:
-
-\begin{verbatim}
-        driver lsi_scsi.o
-\end{verbatim}
-
-\subsection{Bus Bridges}
-
-Currently all bridges supported in the coreboot-v2 tree are transparent
-bridges. This means, once the bridge is initialized, it's remote devices
-are visible on one of the PCI buses without special probing. coreboot
-supports also bridges that are nontransparent.  The driver support code
-can provide a \texttt{scan\_bus} function to scan devices behind the bridge.
-
-\subsection{CPU Reset}
-When changing speed and width of hypertransport chain connections
-coreboot has to either assert an LDTSTOP or a reset to make the changes
-become active.  Additionally Linux can do a firmware reset, if coreboot
-provides the needed infrastructure. To use this capability, define the
-option \texttt{CONFIG\_HAVE\_HARD\_RESET} and add an object file specifying the
-reset code in your mainboard specific configuration file
-\texttt{coreboot-v2/src/mainboard/$<$vendor$>$/$<$mainboard$>$/Config.lb}:
-
-\begin{verbatim}
-        default CONFIG_HAVE_HARD_RESET=1
-        object reset.o
-\end{verbatim}
-
-The C source file \texttt{reset.c} (resulting in \texttt{reset.o}
-during compilation) shall define the following function to take care
-of the system reset:
-
+\label{user name} In ``profile'' section, type the user name for git. This probably can be changed only once.
+{ \small
 \begin{verbatim}
-        void hard_reset(void);
+Profile               Username      zbao
+Preferences           Full Name     Zheng Bao
+Watched Projects      Email Address zheng.bao@amd.com
+Contact Information   Registered    Jun 28, 2011 4:33 PM
+SSH Public Keys       Account ID    1000034
+HTTP Password
+Identities
+Groups
 \end{verbatim}
+}
 
-See \texttt{coreboot-v2/src/mainboard/arima/hdama/reset.c} for an example
-implementation.
-
-\newpage
-
-%
-% 11. coreboot Internals
-%
-
-\section{coreboot Internals}
-This chapter covers some of the internal structures and algorithms of
-coreboot that have not been mentioned so far.
-
-\subsection{Code Flow}
-
-\begin{figure}[htb]
-\centering
-\includegraphics[scale=0.7]{codeflow.pdf}
-\caption{coreboot rough Code Flow}
-\label{fix:codeflow}
-\end{figure}
-
-\newpage
-
-\subsection{Fallback mechanism}
-coreboot provides a mechanism to pack two different coreboot builds
-within one coreboot ROM image. Using the system CMOS memory coreboot
-determines whether the last boot with a default image succeeded and
-boots a failsafe image on failure. This allows insystem testing without
-the risk to render the system unusable. See
-\texttt{coreboot-v2/src/mainboard/arima/hdama/failover.c} for example
-code. The fallback mechanism can be used with the \texttt{cmos\_util}.
-
-\subsection{(Un) Supported Standards}
-coreboot supports the following standards
-\begin{itemize}
-\item Multiprocessing Specification (MPSPEC) 1.4
-\item IRQ Tables (PIRQ)
-\item ACPI (initial support on AMD64)
-\item Elf Booting
-\end{itemize}
-However, the following standards are not supported until now, and will
-probably not be supported in future revisions:
-\begin{itemize}
-\item APM
-\end{itemize}
-
-\subsection{coreboot table}
-coreboot stores information about the system in a data structure called
-the coreboot table. This table can be read under Linux using the tool
-nvramtool from the Lawrence Livermore National Laboratory.
-
-Get more information about lxbios and the utility itself at
-\url{http://www.llnl.gov/linux/lxbios/lxbios.html}
-
-\subsection{ROMCC limitations}
-ROMCC, part of the coreboot project, is a C compiler that translates to
-completely rommable code. This means the resulting code does not need
-any memory to work. This is one of the major improvements in coreboot
-V2, since it allows almost all code to be written in C. DRAM
-initialization can be factored and reused more easily among mainboards
-and platforms.
-
-Since no memory is available during this early initialization point,
-romcc has to map all used variables in registers for the time being.
-Same applies for their stack usage.  Generally the less registers are
-used up by the algorithms, the better code can be factored, resulting in
-a smaller object size. Since getting the best register usage is an NP
-hard problem, some heuristics are used to get reasonable translation
-time. If you run out of registers during compilation, try to refactor
-your code.
-
-\subsection{CMOS handling}
-coreboot can use the mainboard's CMOS memory to store information
-defined in a data structure called the CMOS table . This information
-contains serial line speed, fallback boot control, output verbosity,
-default boot device, ECC control, and more. It can be easily enhanced by
-enhancing the CMOS table. This table, if present, is found at
-\texttt{coreboot-v2/src/mainboard/$<$vendor$>$/$<$mainboard$>$/cmos.layout}.
-It describes the available options, their possible values and their
-position within the CMOS memory. The layout file looks as follows:
+\label{Contact Information} In ``Contact Information'', enter you full name and your Email, which should be configured in your .gitconfig
+{ \small
 \begin{verbatim}
-    # startbit length config configID    name
-    [..]
-           392      3      e        5    baud_rate
-    [..]
-
-    # configid value human readable description
-      5        0     115200
-      5        1      57600
-      5        2      38400
-      5        3      19200
-      5        4       9600
-      5        5       4800
-      5        6       2400
-      5        7       1200
+      Full Name  __________________________________
+Preferred Email  ______________   Registered Email
 
+Save Changes
 \end{verbatim}
+}
 
-To change CMOS values from a running Linux system, use the
-\texttt{cmos\_util}, provided by Linux Networks as part of the coreboot
-utilities suite. Get it at
-\textit{ftp://ftp.lnxi.com/pub/linuxbios/utilities/}
-
-\subsection {Booting Payloads}
-coreboot can load a payload binary from a Flash device or IDE. This
-payload can be a boot loader, like FILO or Etherboot, a kernel image, or
-any other static ELF binary. If you specify a bzImage as the payload,
-the cbfs utility will figure out how to create a coreboot payload from it.
-
-\subsection{Kernel on dhcp/tftp}
-
-One possible scenario during testing is that you keep your kernel (or
-any additional payload) on a different machine on the network. This can
-quickly be done using a DHCP and TFTP server.
-
-Use for example following \texttt{/etc/dhcpd.conf} (adapt to your
-network):
-
-\begin{verbatim}
-    subnet 192.168.1.0 netmask 255.255.255.0 {
-            range 192.168.1.0 192.168.1.31;
-            option broadcastaddress 192.168.1.255;
-    }
-
-    ddnsupdatestyle adhoc;
-
-    host hammer12 {
-            hardware ethernet 00:04:76:EA:64:31;
-            fixedaddress 192.168.1.24;
-            filename "vmlinuz.elf";
-    }
-\end{verbatim}
-
-
-Additionally you have to run a \texttt{tftp} server. You can start one
-using \texttt{inetd}.  To do this, you have to remove the comment from
-the following line in \texttt{/etc/inetd.conf}:
-
+In ``SSH Public Keys'' section, upload your public key.
+{ \small
 \begin{verbatim}
-    tftp dgram udp wait root /usr/sbin/in.tftpd in.tftpd -s /tftpboot
+Status  Algorithm   Key Comment
+
+Delete
+Add SSH Public Key
+ > How to Generate an SSH Key
++--------------------------+
+|                          |
+|                          |
+|                          |
+|                          |
+|                          |
+|                          |
+|                          |
+|                          |
+|                          |
++--------------------------+
+clear       Add  Close
 \end{verbatim}
+}
 
-Then put your kernel image \texttt{vmlinuz.elf} in \texttt{/tftpboot} on
-the \texttt{tftp} server.
-
-
-\newpage
-
-%
-% 12. Advanced Device Initialization Mechanisms
-%
-
-\section{Advanced Device Initialization Mechanisms}
-
-Like software, today's hardware is getting more and more complex. To
-stay flexible many hardware vendors start breaking hardware
-compatibility to old standards like VGA. Thus, VGA is still supported by
-most cards, but emulation has to be enabled by the firmware for the
-device to operate properly.  Also, many expansion cards are small
-discrete systems that have to initialize attached ram, download
-controller firmware and similar. Without this initialization, an
-operating system can not take advantage of the hardware, so there needs
-to be a way to address this issue. There are several alternatives:
-
-\subsection{Native coreboot Support}
-
-For some devices (ie Trident Cyberblade 3d) there is native coreboot
-support This means there is a small driver bound to the PCI id of the
-device that is called after PCI device ressources are allotted.
-
-PROs:
- \begin{itemize}
- \item open source
- \item minimal driver
- \item early control
- \end{itemize}
-
-CONs:
- \begin{itemize}
- \item need an additional driver
- \item viable for onboard devices only
- \item not flexible for pci cards
- \end{itemize}
-
-\subsection{Using Native Linux Support}
-
-A simple way of getting a whole lot of drivers available for coreboot
-is to reuse Linux drivers by putting a Linux kernel to flash. This
-works, because no drivers are needed to get the Linux kernel (as opposed
-to store the kernel on a harddisk connected to isa/scsi/raid storage)
-
-PROs:
- \begin{itemize}
- \item large number of open source drivers
- \end{itemize}
-
-CONs:
- \begin{itemize}
- \item need Linux in Flash (BLOAT!)
- \item drivers expect devices to be initialized (LSI1020/1030)
- \item Linux only
- \item large flash needed (4MBit minimum, normal operations 8+ MBit)
- \end{itemize}
-
-
-\subsection{Running X86 Option ROMs}
-
-Especially SCSI/RAID controllers and graphics adapters come with a
-special option rom. This option rom usually contains x86 binary code
-that uses a legacy PCBIOS interface for device interaction. If this code
-gets executed, the device becomes operable in Linux and other operating
-systems.
-
-PROs:
- \begin{itemize}
- \item really flexible
- \item no need for additional drivers on firmware layer
- \item large number of supported devices
- \end{itemize}
-
-CONs:
- \begin{itemize}
- \item non-x86 platforms need complex emulation
- \item x86 platforms need legacy API
- \item outdated concept
- \end{itemize}
-
-
-\subsection{Running Open Firmware Option ROMs}
-
-Some PCI devices come with open firmware option roms. These devices are
-normally found in computers from SUN, Apple or IBM. Open Firmware is a
-instruction set architecture independent firmware standard that allows
-device specific initialization using simple, small, but flexible
-bytecode that runs with minimal footprint on all architectures that have
-an Open Firmware implementation.
-
-There is a free Open Firmware implementation available, called OpenBIOS,
-that runs on top of coreboot. See www.openbios.org
-
-PROs:
- \begin{itemize}
- \item architecture independence
- \item small footprint
- \item clean concept, less bugs
- \end{itemize}
-
-CONs:
- \begin{itemize}
- \item only small number of devices come with OpenFirmware capable option roms
- \end{itemize}
-
-%
-% 13 image types
-%
-
-\section{Image types}
-There used to be one image type for coreboot, as described above. Since this paper was written (2004) there have been many changes. First, the name
-was changed to coreboot, for many reasons. Second, Cache As Ram support (CAR)
-was added for many AMD CPUs, which both simplified and complicated things. Simplification came with the removal of romcc; complication came with the addition of new ways to build.
-
-There are two big additions to the build process and, furthermore, more than two new CONFIG variables to control them.
-
-\begin{itemize}
-\item \begin{verbatim}CONFIG_USE_DCACHE_RAM\end{verbatim}
-
-Set to \texttt{1} to use Cache As Ram (CAR). Defaults to \texttt{0}
-
-\end{itemize}
-
-Before going over the new image types, derived from v3, we will quickly review the standard v2 image types. We are hoping this review will
-aid comprehension.
-
-A coreboot rom file consists of one or more \textit{images}. All images consist of a part that runs in ROM, and a part that runs in RAM. The RAM can be in  compressed form and is decompressed when needed by the ROM code. The main function of the ROM code is to get memory working. Both ROM and RAM consist of a very small amount of assembly code and mostly C code.
-
-\subsection{romcc images (from emulation/qemu)}
-ROMCC images are so-called because C code for the ROM part is compiled with romcc. romcc is an optimizing C compiler which compiles one, and only
-one file; to get more than one file, one must include the C code via include statements. The main ROM code .c file is usually called auto.c.
-\subsubsection{How it is built}
-Romcc compiles auto.c to produce auto.inc. auto.inc is included in the main crt0.S, which is then preprocessed to produce crt0.s. The inclusion of files into crt0.S is controlled by the CONFIG\_CRT0\_INCLUDES variable. crt0.s is then assembled.
-
-File for the ram part are compiled in a conventional manner.
-
-The final step is linking. The use of named sections is used very heavily in coreboot to control where different bits of code go. The reset vector must go in the top 16 bytes. The start portion of the ROM code must go in the top 64K bytes, since most chipsets only enable this much ROM at startup time. Here is a quick look at a typical image:
+Click ``Add Key ...''
+Go back to you linux command line and type:
+{ \small
 \begin{verbatim}
-  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
-  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
-  [ 1] .ram              PROGBITS        ffff0000 001000 005893 00  WA  0   0  1
-  [ 2] .rom              PROGBITS        ffff5893 006893 00029d 00  AX  0   0 16
-  [ 3] .reset            PROGBITS        fffffff0 006ff0 000010 00   A  0   0  1
-  [ 4] .id               PROGBITS        ffffffd1 006fd1 00001f 00   A  0   0  1
-  [ 5] .shstrtab         STRTAB          00000000 007000 000030 00      0   0  1
-  [ 6] .symtab           SYMTAB          00000000 007170 000c30 10      7  37  4
-  [ 7] .strtab           STRTAB          00000000 007da0 000bfd 00      0   0  1
+$ ssh-keygen
+Generating public/private rsa key pair.
+Enter file in which to save the key (/home/zhengbao/.ssh/id_rsa):
+Enter passphrase (empty for no passphrase):
+Enter same passphrase again:
+Your identification has been saved in /home/zhengbao/.ssh/id_rsa.
+Your public key has been saved in /home/zhengbao/.ssh/id_rsa.pub.
+The key fingerprint is:
+xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx:xx zhengb@host.domain
+The key's randomart image is:
++--[ RSA 2048]----+
+|                 |
+|                 |
+|                 |
+|                 |
+|                 |
+|                 |
+|                 |
+|                 |
+|                 |
++-----------------+
 \end{verbatim}
+}
+The data in ~/.ssh/id\_rsa.pub is your public key. Copy them to the box in the page of ``SSH Public Keys'' and click add.
 
-The only sections that get loaded into a ROM are the Allocated ones. We can see the .ram, .rom, .reset and .id sections.
-\subsubsection{layout}
-As we mentioned, the ROM file consists of multiple images. In the basic file, there are two full coreboot rom images. The build sequence for each is the same, and in fact the ldscript.ld files are almost identical. The only difference is in a few makefile variables, generated by the config tool.
-
-\begin{itemize}
-\item CONFIG\_PAYLOAD\_SIZE. Each image may have a different payload size.
-\item CONFIG\_ROMBASE Each image must have a different base in rom.
-\item CONFIG\_RESET Unclear what this is used for.
-\item CONFIG\_EXCEPTION\_VECTORS where an optional IDT might go.
-\item CONFIG\_USE\_OPTION\_TABLE if set, an option table section will be linked in.
-\item CONFIG\_ROM\_PAYLOAD\_START This is the soon-to-be-deprecated way of locating a payload. cbfs eliminates this.
-\item CONFIG\_USE\_FALLBACK\_IMAGE Whether this is a fallback or normal image
-\item CONFIG\_ROM\_SECTION\_SIZE Essentially, the payload size. Soon to be deprecated.
-\item CONFIG\_ROM\_IMAGE\_SIZE Size of this image (i.e. fallback or normal image)
-\item CONFIG\_ROM\_SIZE Total size of the ROM
-\item CONFIG\_XIP\_RAM\_BASE The start of eXecute In Place code. XIP allows for not copying code to ram, but just running it from ROM.
-\end{itemize}
-
-Each image (normal or fallback) is built completely independently and does not get linked to the other. They are assembled into one ROM image by the (soon to be deprecated) buildrom tool, or by the cbfs tool.
-
-\subsubsection{boot sequence}
-We boot and start at fffffff0. We then jump to the entry point at \_start.  \_start does some machine init and an lgdt and jumps to \_\_protected\_start, at which point we are in protected mode. The code does a bit more machine setup and then starts executing the romcc code.
-
-If fallback has been built in, some setup needs to be done. On some machines, it is extensive. Full rom decoding must be enabled. This may in turn require additional PCI setup to enable decoding to be enabled (!). To decided which image to use, hardware registers (cold boot on the Opteron) or CMOS are checked. Finally, once the image to use has been decided, a jmp is performed, viz:
-\begin{verbatim}
-        /* This is the primary cpu how should I boot? */
-        else if (do_normal_boot()) {
-                goto normal_image;
-        }
-        else {
-                goto fallback_image;
-        }
- normal_image:
-        __asm__ volatile ("jmp __normal_image"
-                : /* outputs */
-                : "a" (bist), "b" (cpu_init_detectedx) /* inputs */
-                );
-
- fallback_image:
-#if CONFIG_HAVE_FAILOVER_BOOT==1
-        __asm__ volatile ("jmp __fallback_image"
-                : /* outputs */
-                : "a" (bist), "b" (cpu_init_detectedx) /* inputs */
-                )
-#endif
-        ;
-\end{verbatim}
-How does the fallback image get the symbol for normal entry? Via magic in the ldscript.ld -- remember, the images are not linked to each other.
-Finally, we can see this in the Config.lb for most mainboards:
-\begin{verbatim}
-if CONFIG_USE_FALLBACK_IMAGE
-        mainboardinit cpu/x86/16bit/reset16.inc
-        ldscript /cpu/x86/16bit/reset16.lds
-else
-        mainboardinit cpu/x86/32bit/reset32.inc
-        ldscript /cpu/x86/32bit/reset32.lds
-end
-\end{verbatim}
-What does this mean? the non-fallback image has a 32-bit entry point; fallback has a 16-bit entry point. The reason for this is that some code from fallback always runs, so as to pick fallback or normal; but the normal is always called from 32-bit code.
-\subsection{car images (from lippert/roadrunner-lx)}
-CAR images in their simplest form are modified romcc images. The file is usually cache\_as\_ram\_auto.c. C inclusion is still used. The main difference is in the build sequence. The compiler command line is a very slight changed: instead of using romcc to generate an auto.inc include file, gcc us used. Then, two perl scripts are used to rename the .text and .data sections to .rom.text and .rom.data respectively.
-\subsubsection{How it is built}
-The build is almost identical to the romcc build. Since the auto.inc file exists, it can be included as before. The crt0\_includes.h file has one addition: a file that enables CAR, in this case it is \textit{src/cpu/amd/model\_lx/cache\_as\_ram.inc}.
-\subsubsection{layout}
-No significant change from romcc code.
-\subsubsection{boot sequence}
-No significant change from romcc code, except that the CAR code has to set up a stack.
-
-\subsection{car + CONFIG\_USE\_INIT images (new emulation/qemu}
-This type of image makes more use of the C compiler. In this type of image, in fact,
-seperate compilation is possible but is not always used. Oddly enough, this option is only used in PPC boards. That said, we need to move to this way of building. Including C code is poor style.
-\subsubsection{How it is built}
-There is a make variable, INIT-OBJECTS, that for all our other targets is empty. In this type of build, INIT-OBJECTS is a list of C files that are created from the config tool initobject command. Again, with INIT-OBJECTS we can finally stop including .c files and go with seperate compilation.
-\subsubsection{layout}
-No significant change from romcc code.
-\subsubsection{boot sequence}
-No significant change from romcc code, except that the CAR code has to set up a stack.
-
-\subsubsection{layout}
-No significant change from romcc code.
-\subsubsection{boot sequence}
-No significant change from romcc code, except that the CAR code has to set up a stack.
-\subsection{failover}
-Failover is the newest way to lay out a ROM. The choice of which image to run is removed from the fallback image and moved into a small, standalone piece of code. The code is simple enough to show here:
+In ``HTTP Password'' section, click button ``Generate Password''. You will get the password for http checkout.
+{ \small
 \begin{verbatim}
-static unsigned long main(unsigned long bist)
-{
-	if (do_normal_boot())
-		goto normal_image;
-	else
-		goto fallback_image;
+Username    XXX
+Password    XXXXXXXXXXXX
 
-normal_image:
-	__asm__ __volatile__("jmp __normal_image" : : "a" (bist) : );
-
-cpu_reset:
-	__asm__ __volatile__("jmp __cpu_reset" : : "a" (bist) : );
-
-fallback_image:
-	return bist;
-}
+Generate Password   Clear Password
 
 \end{verbatim}
-Some motherboards have a more complex bus structure (e.g. Opteron). In those cases, the failover can be more complex, as it requires some hardware initialization to work correctly. As of this writing (April 2009), these boards have their own failover:
-\begin{quote}
-./src/mainboard/iei/nova4899r/failover.c
-./src/mainboard/emulation/qemu-x86/failover.c
-./src/mainboard/supermicro/x6dhr\_ig/failover.c
-./src/mainboard/supermicro/x6dai\_g/failover.c
-./src/mainboard/supermicro/x6dhe\_g2/failover.c
-./src/mainboard/supermicro/x6dhr\_ig2/failover.c
-./src/mainboard/supermicro/x6dhe\_g/failover.c
-./src/mainboard/dell/s1850/failover.c
-./src/mainboard/intel/xe7501devkit/failover.c
-./src/mainboard/intel/jarrell/failover.c
-./src/mainboard/olpc/btest/failover.c
-./src/mainboard/olpc/rev\_a/failover.c
-./src/mainboard/via/epia-m/failover.c
-\end{quote}
-Here is one of the more complicated ones:
-\begin{verbatim}
-static unsigned long main(unsigned long bist)
-{
-        /* Did just the cpu reset? */
-        if (memory_initialized()) {
-                if (last_boot_normal()) {
-                        goto normal_image;
-                } else {
-                        goto cpu_reset;
-                }
-        }
-
-        /* This is the primary cpu how should I boot? */
-        else if (do_normal_boot()) {
-                goto normal_image;
-        }
-        else {
-                goto fallback_image;
-        }
- normal_image:
-        asm volatile ("jmp __normal_image"
-                : /* outputs */
-                : "a" (bist) /* inputs */
-                : /* clobbers */
-                );
- cpu_reset:
-        asm volatile ("jmp __cpu_reset"
-                : /* outputs */
-                : "a"(bist) /* inputs */
-                : /* clobbers */
-                );
- fallback_image:
-        return bist;
 }
 
-\end{verbatim}
-They're not that different, in fact. So why are there different copies all over the tree? Simple: code inclusion. Most of the failover.c are different because they include different bits of code. Here is a key reason for killing C code inclusion in the tree.
-\subsubsection{How it is built}
-There two additional config variables:
-\begin{itemize}
-\item HAVE\_FAILOVER\_IMAGE Has to be defined when certain files are included.
-\item USE\_FAILOVER\_IMAGE Enables the use of the failover image
-\end{itemize}
-Confusingly enough, almost all the uses of these two variables are either nested or both required to be set, e.g.
-The fallback and normal builds are the same. The target config has a new clause that looks like this:
-\begin{verbatim}
-romimage "failover"
-        option CONFIG_USE_FAILOVER_IMAGE=1
-        option CONFIG_USE_FALLBACK_IMAGE=0
-        option CONFIG_ROM_IMAGE_SIZE=CONFIG_FAILOVER_SIZE
-        option CONFIG_XIP_ROM_SIZE=CONFIG_FAILOVER_SIZE
-        option COREBOOT_EXTRA_VERSION="\$(shell cat ../../VERSION)\_Failover"
-end
-\end{verbatim}
-This new section uses some constructs not yet discussed in detail. XIP\_ROM\_SIZE just refers to the
-fact that the failover code is eXecute In Place, i.e. not copied to RAM. Of course, the ROM part of normal/fallback is as well, so the usage of XIP here is somewhat confusing. Finally, the USE\_FAILOVER\_IMAGE variable is set, which changes code compilation in a few places. If we just consider non-mainbard files, there are:
-\begin{verbatim}
-src/cpu/amd/car/cache_as_ram.inc
-src/arch/i386/Config.lb
-\end{verbatim}
-For the cache\_as\_ram.inc file, the changes relate to the fact that failover code sets up CAR, so that fallback code need not.
-
-For the Config.lb, several aspects of build change.
-When USE\_FAILOVER\_IMAGE, entry into both normal and fallback bios images is via a 32-bit entry point (when not defined, entry into fallback is a 16-entry point at the power-on reset vector).
-\subsubsection{layout}
-Failover.c becomes the new bootblock at the top of memory. It calls either normal or fallback. The address of normal and fallback is determined by ldscript magic.
-\subsubsection{boot sequence}
-failover.c tests a few variables and the calls the normal or fallback payload depending on those variables; usually they are CMOS settings.
-\subsection{Proposed new image forat}
-The new image format will use seperate compilation -- no C code included! -- on all files.
-
-The new design has a few key goals:
-\begin{itemize}
-\item Always use a bootblock (currently called failover).
-The name failover.c, being utterly obscure, will not be used; instead, we will name the file bootblock.c. Instead of having a different copy for each mainboard, we can have just one copy.
-\item Always use seperate compilation
-\item Always use printk etc. in the ROM code
-\item (longer term) from the bootblock, always use cbfs to locate the normal/fallback etc. code. This code will be XIP.
-\end{itemize}
+\subsection{Reviewing Changes}
+For each listed changes in Gerrit, you can review, comment, evaluate,
+cherry-pick, and even re-submit them. For you own patches, only you can
+abandon them. Click in the file and commit message, you can add in-line comment.
 
-\subsubsection{How it is built}
-For now, since we are still using the config tool, we'll need a new command: bootblockobject, which creates a list of files to be included in the bootblock.   Not a lot else will have to change. We are going to move to using the v3 CAR code assembly code (one or two files at most, instead of many) and, instead of the thicket of little ldscript files, one ldscript file. This strategy is subject to modification as events dictate.
-\subsubsection{layout}
-Almost the same, for now, as the current failover code.
-\subsubsection{boot sequence}
 %
 % 14 Glossary
 %
@@ -1766,6 +627,21 @@ pure initialization.
 
 Flash devices are commonly used in all different computers since unlike
 ROMs they can be electronically erased and reprogrammed.
+
+\item Gerrit
+
+Gerrit is a web based code review system, facilitating online code
+reviews for projects using the Git version control system.
+
+Gerrit makes reviews easier by showing changes in a side-by-side
+display, and allowing inline comments to be added by any reviewer.
+
+Gerrit simplifies Git based project maintainership by permitting any
+authorized user to submit changes to the master Git repository, rather
+than requiring all approved changes to be merged in by hand by the
+project maintainer. This functionality enables a more centralized
+usage of Git.
+
 \end{itemize}
 
 \newpage
@@ -1780,18 +656,16 @@ ROMs they can be electronically erased and reprogrammed.
 \begin{itemize}
  \item
  \textit{\url{http://www.coreboot.org/Documentation}}
- \item
- \textit{\url{http://www.lysator.liu.se/upplysning/fa/linuxbios.pdf}}
- \item
- \textit{\url{http://portal.acm.org/citation.cfm?id=512627}}
 \end{itemize}
 
 \subsection {Links}
 
 \begin{itemize}
  \item Etherboot: \textit{\url{http://www.etherboot.org/}}
- \item Filo: \textit{\url{http://www.coreboot.org/FILO}}
  \item OpenBIOS: \textit{\url{http://www.openbios.org/}}
+ \item Flashrom: \textit{\url{http://www.flashrom.org/}}
+ \item Seabios: \textit{\url{http://www.seabios.org/}}
 \end{itemize}
 
+
 \end{document}
-- 
cgit v1.2.3

