From 879c17784f88994c03e90aca85710d7aac6582de Mon Sep 17 00:00:00 2001
From: Myles Watson <mylesgw@gmail.com>
Date: Tue, 25 Aug 2009 19:46:50 +0000
Subject: Correct typos /subdir/subdirs/ in documentation and
 util/x86emu/Makefile.inc.

Signed-off-by: Myles Watson <mylesgw@gmail.com>
Acked-by: Myles Watson <mylesgw@gmail.com>


git-svn-id: svn://svn.coreboot.org/coreboot/trunk@4582 2b7e53f0-3cfb-0310-b3e9-8179ed1497e1
---
 documentation/Kconfig.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'documentation/Kconfig.tex')

diff --git a/documentation/Kconfig.tex b/documentation/Kconfig.tex
index 25f54621b5..32fdd19ec5 100644
--- a/documentation/Kconfig.tex
+++ b/documentation/Kconfig.tex
@@ -21,8 +21,8 @@ Kconfig files use the source command to include subdirectories. In most cases, s
 There is only one Makefile, at the top level. All other makefiles are included as Makefile.inc. All the next-level Makefile.inc files are selected in the top level Makefile. Directories that are platform-independent are in BUILD-y; platform-dependent (e.g. Makefile.inc's that depend on architecture) are included in PLATFORM-y.
 
 Make is not recursive. There is only one make process.
-\subsection{subdir usage}
-Further includes of Makefile.inc, if needed, are done via subdir-y commands. As in Linux, the subdir can be conditional or unconditional. Conditional includes are done via subdir-\$(CONFIG\_VARIABLE) usage; unconditional are done via subdir-y.
+\subsection{subdirs usage}
+Further includes of Makefile.inc, if needed, are done via subdirs-y commands. As in Linux, the subdirs can be conditional or unconditional. Conditional includes are done via subdirs-\$(CONFIG\_VARIABLE) usage; unconditional are done via subdirs-y.
 
 We define the common rules for which variation to use below.
 \subsection{object file specification}
-- 
cgit v1.2.3

